AR15 variants:

Front sight posts:
    *
      Windage:   

  *
     Elevation:   

A1 20” = 1 MOA
    *
A1 20” = 1 MOA
  *
A2 20” = 1 MOA

A1 16” = 1.5 MOA
    *
A1 16” = 1.5 MOA
  *
A2 16” = 1.5 MOA

A2&3 20” = 1.25 MOA      *
A2&3 20” = ½ MOA
  *
A3 20” = ½ MOA

A2&3 16” = 1.875 MOA    *
A2&3 16” = ¾ MOA
  *
A3 16” = ¾ MOA

** If zeroed at 25m with small aperture, zero is for 300m, large aperture is 200m

-------------------------------------------------------------------------------------------------

SKS/ AK

Front Sight Elevation:    8 MOA per turn

Front Sight Windage:     Approx 1 MOA per .006” (Drift tool is approx .035” per turn)

Rear Sight Elevation:     Approx 3 MOA per detent out to 300m

-------------------------------------------------------------------------------------------------

SOCOM M1A

Rear sight elevation =  1.5 MOA?     Rear sight windage =  1.5 MOA?

-------------------------------------------------------------------------------------------------

FAL

Front sight:  ?

Rear Sight:   ?
-------------------------------------------------------------------------------------------------

10/22 w/ Tech- Sights:     
                                                 22” Barrel              20” Barrel            18” Barrel                16"  Barrel
Front Sight Elevation:   .375 MOA/click1     .5 MOA/click        .625 MOA/click2        .75 MOA/click
Rear Sight Elevation:     .375 MOA/click1     .5 MOA/click        .625 MOA/click2        .75 MOA/click
Rear Sight Windage:      .375 MOA/click1     .5 MOA/click        .625 MOA/click2        .75 MOA/click

1.  This is 3/8 MOA/click, or 3 MOA per 8 clicks
2.  This is 5/8 MOA/click, or 5 MOA per 8 clicks
---------------------------------------------------------------------------------------------------
Ruger Mini 14

Windage= 1 MOA

Elevation= 1 MOA

---------------------------------------------------------------------------------------------------

HK 91
Windage & elevation = 1.25 MOA per turn of the drum

-------------------------------------------------------------------------------------------------

HK93 

Windage & elevation = 1.6 MOA per turn of the drum
-------------------------------------------------------------------------------------------------
Steyr AUG 

Windage & elevation = 1.5 MOA per click
