Front sight posts: *Rear Sight Windage: * Rear Sight Elevation: 
A1 20 = 1 MOA * A1 20 = 1 MOA * A2 20 = 1 MOA 
A1 16 = 1.5 MOA * A1 16 = 1.5 MOA * A2 16 = 1.5 MOA 

[bookmark: _GoBack]A2&3 20 = 1.25 MOA * A2&3 20 = ½ MOA * A3 20 = ½ MOA 
A2&3 16 = 1.875 MOA * A2&3 16 = ¾ MOA * A3 16 = ¾ MOA 
If zeroed at 25m with small aperture, zero is for 300m, large aperture is 200m 
------------------------------------------------------------------------------------------------- 
SKS/ AK 
Front Sight Elevation: 8 MOA per turn (4 MOA per half turn, 2 MOA per quarter turn) 
Front Sight Windage: Approx 1 MOA per .006 (Drift tool is approx .035 per turn) 
Rear Sight Elevation: Approx 3 MOA per detent out to 300m 
------------------------------------------------------------------------------------------------- 
SOCOM (Short Barreled) M1A 
Rear sight elevation = 1.5 MOA? Rear sight windage = 1.5 MOA? 
------------------------------------------------------------------------------------------------- 
FAL (Std. 21 barrel) 
Front sight: 6 MOA per turn (3 MOA per half turn, 1.5 MOA per quarter turn) 
Rear Sight: Trial & Error in the 200 position 
------------------------------------------------------------------------------------------------- 
10/22 w/ Tech- Sights: 22� Barrel 20� Barrel 18� Barrel 16"  
Front Sight Elevation: .375 MOA/click   .5 MOA/click   .625 MOA/click   .75 MOA/click 
Rear Sight Elevation: .375 MOA/click   .5 MOA/click   .625 MOA/click   .75 MOA/click 
Rear Sight Windage: .375 MOA/click   .5 MOA/click   .625 MOA/click   .75 MOA/click  
This is 3/8 MOA/click, or 3 MOA per 8 clicks 2. This is 5/8 MOA/click, or 5 MOA per 8 clicks 
--------------------------------------------------------------------------------------------------- 
Ruger Mini 14 
Windage= 1 MOA 
Elevation= 1 MOA 
--------------------------------------------------------------------------------------------------- 
HK 91 
Windage & elevation = 1.25 MOA per turn of the drum 
------------------------------------------------------------------------------------------------- 
HK93 
Windage & elevation = 1.6 MOA per turn of the drum 
------------------------------------------------------------------------------------------------- 
Steyr AUG 
Windage & elevation = 1.5 MOA per click
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